MILKDROP_PRESET_VERSION=201
PSVERSION=2
PSVERSION_WARP=2
PSVERSION_COMP=2
[preset00]
fRating=5.000000
fGammaAdj=2.000
fDecay=0.980
fVideoEchoZoom=2.000
fVideoEchoAlpha=0.000
nVideoEchoOrientation=0
nWaveMode=7
bAdditiveWaves=1
bWaveDots=0
bWaveThick=0
bModWaveAlphaByVolume=1
bMaximizeWaveColor=0
bTexWrap=0
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=0
bDarken=0
bSolarize=0
bInvert=0
fWaveAlpha=0.001
fWaveScale=1.286
fWaveSmoothing=0.630
fWaveParam=0.000
fModWaveAlphaStart=0.710
fModWaveAlphaEnd=1.300
fWarpAnimSpeed=0.010
fWarpScale=100.000
fZoomExponent=0.19890
fShader=0.000
zoom=1.00000
rot=0.00000
cx=0.500
cy=0.500
dx=0.00001
dy=0.00001
warp=0.17914
sx=1.00000
sy=1.00000
wave_r=0.650
wave_g=0.650
wave_b=0.650
wave_x=0.500
wave_y=0.500
ob_size=0.005
ob_r=0.000
ob_g=0.000
ob_b=0.000
ob_a=1.000
ib_size=0.000
ib_r=0.250
ib_g=0.250
ib_b=0.250
ib_a=0.000
nMotionVectorsX=64.000
nMotionVectorsY=48.000
mv_dx=0.000
mv_dy=0.000
mv_l=0.000
mv_r=1.000
mv_g=1.000
mv_b=1.000
mv_a=0.000
b1n=0.000
b2n=0.000
b3n=0.000
b1x=1.000
b2x=1.000
b3x=1.000
b1ed=0.250
wavecode_0_enabled=1
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=0
wavecode_0_bUseDots=0
wavecode_0_bDrawThick=1
wavecode_0_bAdditive=0
wavecode_0_scaling=1.00000
wavecode_0_smoothing=0.50000
wavecode_0_r=1.000
wavecode_0_g=1.000
wavecode_0_b=1.000
wavecode_0_a=1.000
wave_0_per_point1=ma=ma+(above(bass,1)*3.1415*.01*bass);
wave_0_per_point2=ma=ma-(above(treb,1)*3.1415*.01*treb);
wave_0_per_point3=
wave_0_per_point4=mx=mx+(.0002*cos(ma));
wave_0_per_point5=my=my+(.0002*sin(ma));
wave_0_per_point6=
wave_0_per_point7=mx=if(above(mx,.9),(.9-mx),mx);
wave_0_per_point8=my=if(above(my,.9),(.9-my),my);
wave_0_per_point9=mx=if(below(mx,.1),(.9+mx),mx);
wave_0_per_point10=my=if(below(my,.1),(.9+my),my);
wave_0_per_point11=
wave_0_per_point12=x=mx;
wave_0_per_point13=y=my;
wave_0_per_point14=
wave_0_per_point15=a=(above(bass+mid+treb,.8));
wave_0_per_point16=pi23=4*asin(1)*.333333333;
wave_0_per_point17=vol=bass+mid+treb;
wave_0_per_point18=r=(sin(time*.3+vol-0*pi23)+1)*.5;
wave_0_per_point19=g=(sin(time*.3+vol-1*pi23)+1)*.5;
wave_0_per_point20=b=(sin(time*.3+vol-2*pi23)+1)*.5;
wavecode_1_enabled=1
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=0
wavecode_1_bUseDots=0
wavecode_1_bDrawThick=1
wavecode_1_bAdditive=0
wavecode_1_scaling=1.00000
wavecode_1_smoothing=0.50000
wavecode_1_r=1.000
wavecode_1_g=1.000
wavecode_1_b=1.000
wavecode_1_a=1.000
wave_1_per_point1=ma=ma+(above(bass,1)*3.1415*.05*bass);
wave_1_per_point2=ma=ma-(above(mid,1)*3.1415*.05*mid);
wave_1_per_point3=
wave_1_per_point4=mx=mx+(.0001*cos(ma));
wave_1_per_point5=my=my+(.0001*sin(ma));
wave_1_per_point6=
wave_1_per_point7=mx=if(above(mx,.9),(.9-mx),mx);
wave_1_per_point8=my=if(above(my,.9),(.9-my),my);
wave_1_per_point9=mx=if(below(mx,.1),(.9+mx),mx);
wave_1_per_point10=my=if(below(my,.1),(.9+my),my);
wave_1_per_point11=
wave_1_per_point12=x=mx;
wave_1_per_point13=y=my;
wave_1_per_point14=
wave_1_per_point15=a=(above(bass+mid+treb,.1));
wave_1_per_point16=pi23=4*asin(1)*.333333333;
wave_1_per_point17=vol=bass+mid+treb;
wave_1_per_point18=r=(sin(time*.3+vol-0*pi23)+1)*.5;
wave_1_per_point19=g=(sin(time*.3+vol-1*pi23)+1)*.5;
wave_1_per_point20=b=(sin(time*.3+vol-2*pi23)+1)*.5;
wavecode_2_enabled=1
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=0
wavecode_2_bUseDots=1
wavecode_2_bDrawThick=1
wavecode_2_bAdditive=0
wavecode_2_scaling=1.00000
wavecode_2_smoothing=0.50000
wavecode_2_r=1.000
wavecode_2_g=1.000
wavecode_2_b=1.000
wavecode_2_a=1.000
wave_2_per_point1=ma=ma+(above(mid,1)*3.1415*.01*mid);
wave_2_per_point2=ma=ma-(above(treb,1)*3.1415*.01*treb);
wave_2_per_point3=
wave_2_per_point4=mx=mx+(.0004*cos(ma));
wave_2_per_point5=my=my+(.0004*sin(ma));
wave_2_per_point6=
wave_2_per_point7=mx=if(above(mx,.9),(.9-mx),mx);
wave_2_per_point8=my=if(above(my,.9),(.9-my),my);
wave_2_per_point9=mx=if(below(mx,.1),(.9+mx),mx);
wave_2_per_point10=my=if(below(my,.1),(.9+my),my);
wave_2_per_point11=
wave_2_per_point12=x=mx;
wave_2_per_point13=y=my;
wave_2_per_point14=
wave_2_per_point15=a=(above(bass+mid+treb,.3));
wave_2_per_point16=pi23=4*asin(1)*.333333333;
wave_2_per_point17=vol=bass+mid+treb;
wave_2_per_point18=r=(sin(time*.3+vol-0*pi23)+1)*.5;
wave_2_per_point19=g=(sin(time*.3+vol-1*pi23)+1)*.5;
wave_2_per_point20=b=(sin(time*.3+vol-2*pi23)+1)*.5;
wavecode_3_enabled=1
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=0
wavecode_3_bUseDots=0
wavecode_3_bDrawThick=1
wavecode_3_bAdditive=0
wavecode_3_scaling=1.00000
wavecode_3_smoothing=0.50000
wavecode_3_r=1.000
wavecode_3_g=1.000
wavecode_3_b=1.000
wavecode_3_a=1.000
wave_3_per_point1=ma=ma+(above(bass,.5)*3.1415*.02*bass);
wave_3_per_point2=ma=ma-(above(treb,.5)*3.1415*.02*treb);
wave_3_per_point3=
wave_3_per_point4=mx=mx+(.0008*cos(ma));
wave_3_per_point5=my=my+(.0008*sin(ma));
wave_3_per_point6=
wave_3_per_point7=mx=if(above(mx,.9),(.9-mx),mx);
wave_3_per_point8=my=if(above(my,.9),(.9-my),my);
wave_3_per_point9=mx=if(below(mx,.1),(.9+mx),mx);
wave_3_per_point10=my=if(below(my,.1),(.9+my),my);
wave_3_per_point11=
wave_3_per_point12=x=mx;
wave_3_per_point13=y=my;
wave_3_per_point14=
wave_3_per_point15=a=(above(bass+mid+treb,.2));
wave_3_per_point16=pi23=4*asin(1)*.333333333;
wave_3_per_point17=vol=bass+mid+treb;
wave_3_per_point18=r=(sin(time*.3+vol-0*pi23)+1)*.5;
wave_3_per_point19=g=(sin(time*.3+vol-1*pi23)+1)*.5;
wave_3_per_point20=b=(sin(time*.3+vol-2*pi23)+1)*.5;
shapecode_0_enabled=0
shapecode_0_sides=4
shapecode_0_additive=0
shapecode_0_thickOutline=0
shapecode_0_textured=1
shapecode_0_num_inst=1
shapecode_0_x=0.500
shapecode_0_y=0.500
shapecode_0_rad=1.79142
shapecode_0_ang=0.00000
shapecode_0_tex_ang=0.62832
shapecode_0_tex_zoom=1.00000
shapecode_0_r=1.000
shapecode_0_g=1.000
shapecode_0_b=1.000
shapecode_0_a=0.000
shapecode_0_r2=0.000
shapecode_0_g2=0.000
shapecode_0_b2=0.000
shapecode_0_a2=1.000
shapecode_0_border_r=1.000
shapecode_0_border_g=1.000
shapecode_0_border_b=1.000
shapecode_0_border_a=0.000
shapecode_1_enabled=0
shapecode_1_sides=4
shapecode_1_additive=0
shapecode_1_thickOutline=0
shapecode_1_textured=0
shapecode_1_num_inst=1
shapecode_1_x=0.500
shapecode_1_y=0.500
shapecode_1_rad=0.10000
shapecode_1_ang=0.00000
shapecode_1_tex_ang=0.00000
shapecode_1_tex_zoom=1.00000
shapecode_1_r=1.000
shapecode_1_g=0.000
shapecode_1_b=0.000
shapecode_1_a=1.000
shapecode_1_r2=0.000
shapecode_1_g2=1.000
shapecode_1_b2=0.000
shapecode_1_a2=0.000
shapecode_1_border_r=1.000
shapecode_1_border_g=1.000
shapecode_1_border_b=1.000
shapecode_1_border_a=0.100
shapecode_2_enabled=0
shapecode_2_sides=4
shapecode_2_additive=0
shapecode_2_thickOutline=0
shapecode_2_textured=0
shapecode_2_num_inst=1
shapecode_2_x=0.500
shapecode_2_y=0.500
shapecode_2_rad=0.10000
shapecode_2_ang=0.00000
shapecode_2_tex_ang=0.00000
shapecode_2_tex_zoom=1.00000
shapecode_2_r=1.000
shapecode_2_g=0.000
shapecode_2_b=0.000
shapecode_2_a=1.000
shapecode_2_r2=0.000
shapecode_2_g2=1.000
shapecode_2_b2=0.000
shapecode_2_a2=0.000
shapecode_2_border_r=1.000
shapecode_2_border_g=1.000
shapecode_2_border_b=1.000
shapecode_2_border_a=0.100
shapecode_3_enabled=0
shapecode_3_sides=4
shapecode_3_additive=0
shapecode_3_thickOutline=0
shapecode_3_textured=0
shapecode_3_num_inst=1
shapecode_3_x=0.500
shapecode_3_y=0.500
shapecode_3_rad=0.10000
shapecode_3_ang=0.00000
shapecode_3_tex_ang=0.00000
shapecode_3_tex_zoom=1.00000
shapecode_3_r=1.000
shapecode_3_g=0.000
shapecode_3_b=0.000
shapecode_3_a=1.000
shapecode_3_r2=0.000
shapecode_3_g2=1.000
shapecode_3_b2=0.000
shapecode_3_a2=0.000
shapecode_3_border_r=1.000
shapecode_3_border_g=1.000
shapecode_3_border_b=1.000
shapecode_3_border_a=0.100
per_frame_1=myVolume = (bass+treb+mid)/3;
per_frame_2=wave_r = wave_r + 0.5*sin(7*bass)*3.78*time;
per_frame_3=wave_b = wave_b + 0.5*sin(7*treb)*6.56*time;
per_frame_4=wave_g = wave_g + 0.5*sin(7*mid)*4.35*time;
per_frame_5=wave_x = wave_x + 0.1*sin(0.89*time);
per_frame_6=wave_y = wave_y + 0.1*sin(0.76*time);
per_frame_7=ob_r = ob_r + 1.5*sin(7*bass)*3.78*time;
per_frame_8=ob_b = ob_b + 1.5*sin(7*treb)*6.56*time;
per_frame_9=ob_g = ob_g + 1.5*sin(7*mid)*4.35*time;
per_frame_10=dy = -0.008 * sin(0.5*time);
per_frame_11=dx = -0.008*  cos(0.26*time);
per_pixel_1=rot = rot + if (below(rad,0.4+ 0.2*sin(bass/mid)), abs(0.02*abs(bass/treb)*sin(time)+ 0.01*abs(mid/treb/bass))*cos(time), 0);
warp_1=`shader_body
warp_2=`{
warp_3=`uv = lerp(uv_orig,uv,0.3);
warp_4=`
warp_5=`float2 d = texsize.zw * 3;
warp_6=`float3 dx = ( GetBlur1(uv + float2(1,0)*d) - GetBlur1(uv-float2(1,0)*d) );
warp_7=`float3 dy = ( GetBlur1(uv + float2(0,1)*d) - GetBlur1(uv-float2(0,1)*d) );
warp_8=`
warp_9=`uv += float2(lum(dx),lum(dy))*texsize.zw*9;
warp_10=`ret = tex2d(sampler_fc_main, uv) - 0.01;
warp_11=`
warp_12=`}
comp_1=`shader_body
comp_2=`{
comp_3=`
comp_4=`uv = 0.5 + (uv-0.5)*0.98;
comp_5=`    float2 d = texsize.zw*4;
comp_6=`    float3 dx = ( GetBlur1(uv+float2(1,0)*d)-GetBlur1(uv-float2(1,0)*d) );
comp_7=`    float3 dy = ( GetBlur1(uv+float2(0,1)*d)-GetBlur1(uv-float2(0,1)*d) );
comp_8=`
comp_9=`float4 noise = tex3D(sampler_noisevol_hq, ((uv.xyy+float3(lum(dx),lum(dy),0)*0.5)*texsize.xyy*texsize_noisevol_hq.zww).xyz*float3(1,1,0)*0.05
comp_10=`                                        + time*float3(0,0,1)*0.2 );
comp_11=`uv -= float2(lum(dx),lum(dy))*0.04;
comp_12=`ret = abs(GetPixel(uv)+GetBlur1(uv)-GetBlur2(uv)-GetBlur3(uv));
comp_13=`ret *= lum(noise)*3; 
comp_14=`ret = pow(ret,0.5);
comp_15=`}
