MILKDROP_PRESET_VERSION=201
PSVERSION=2
PSVERSION_WARP=2
PSVERSION_COMP=2
[preset00]
fRating=5.000000
fGammaAdj=2.000
fDecay=1.000
fVideoEchoZoom=1.000
fVideoEchoAlpha=0.500
nVideoEchoOrientation=0
nWaveMode=7
bAdditiveWaves=1
bWaveDots=0
bWaveThick=0
bModWaveAlphaByVolume=1
bMaximizeWaveColor=0
bTexWrap=1
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=0
bDarken=0
bSolarize=0
bInvert=1
fWaveAlpha=0.001
fWaveScale=1.286
fWaveSmoothing=0.630
fWaveParam=0.000
fModWaveAlphaStart=0.710
fModWaveAlphaEnd=1.300
fWarpAnimSpeed=1.000
fWarpScale=0.267
fZoomExponent=1.00000
fShader=0.000
zoom=1.16000
rot=-0.04000
cx=0.500
cy=0.500
dx=0.00000
dy=0.00000
warp=0.00052
sx=1.00000
sy=1.00000
wave_r=0.650
wave_g=0.650
wave_b=0.650
wave_x=0.500
wave_y=0.500
ob_size=0.010
ob_r=1.000
ob_g=1.000
ob_b=1.000
ob_a=0.000
ib_size=0.010
ib_r=0.250
ib_g=0.250
ib_b=0.250
ib_a=0.000
nMotionVectorsX=64.000
nMotionVectorsY=48.000
mv_dx=0.000
mv_dy=0.000
mv_l=0.000
mv_r=1.000
mv_g=1.000
mv_b=1.000
mv_a=0.000
b1n=0.000
b2n=0.000
b3n=0.000
b1x=1.000
b2x=1.000
b3x=1.000
b1ed=0.250
wavecode_0_enabled=1
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=0
wavecode_0_bUseDots=0
wavecode_0_bDrawThick=1
wavecode_0_bAdditive=0
wavecode_0_scaling=1.00000
wavecode_0_smoothing=0.50000
wavecode_0_r=1.000
wavecode_0_g=1.000
wavecode_0_b=1.000
wavecode_0_a=1.000
wave_0_per_point1=ma=ma+(above(bass,1)*3.1415*.01*bass);
wave_0_per_point2=ma=ma-(above(treb,1)*3.1415*.01*treb);
wave_0_per_point3=
wave_0_per_point4=mx=mx+(.0002*cos(ma));
wave_0_per_point5=my=my+(.0002*sin(ma));
wave_0_per_point6=
wave_0_per_point7=mx=if(above(mx,.9),(.9-mx),mx);
wave_0_per_point8=my=if(above(my,.9),(.9-my),my);
wave_0_per_point9=mx=if(below(mx,.1),(.9+mx),mx);
wave_0_per_point10=my=if(below(my,.1),(.9+my),my);
wave_0_per_point11=
wave_0_per_point12=x=mx;
wave_0_per_point13=y=my;
wave_0_per_point14=
wave_0_per_point15=a=(above(bass+mid+treb,.8));
wave_0_per_point16=pi23=4*asin(1)*.333333333;
wave_0_per_point17=vol=bass+mid+treb;
wave_0_per_point18=r=(sin(time*.3+vol-0*pi23)+1)*.5;
wave_0_per_point19=g=(sin(time*.3+vol-1*pi23)+1)*.5;
wave_0_per_point20=b=(sin(time*.3+vol-2*pi23)+1)*.5;
wavecode_1_enabled=1
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=0
wavecode_1_bUseDots=0
wavecode_1_bDrawThick=1
wavecode_1_bAdditive=0
wavecode_1_scaling=1.00000
wavecode_1_smoothing=0.50000
wavecode_1_r=1.000
wavecode_1_g=1.000
wavecode_1_b=1.000
wavecode_1_a=1.000
wave_1_per_point1=ma=ma+(above(bass,1)*3.1415*.05*bass);
wave_1_per_point2=ma=ma-(above(mid,1)*3.1415*.05*mid);
wave_1_per_point3=
wave_1_per_point4=mx=mx+(.0001*cos(ma));
wave_1_per_point5=my=my+(.0001*sin(ma));
wave_1_per_point6=
wave_1_per_point7=mx=if(above(mx,.9),(.9-mx),mx);
wave_1_per_point8=my=if(above(my,.9),(.9-my),my);
wave_1_per_point9=mx=if(below(mx,.1),(.9+mx),mx);
wave_1_per_point10=my=if(below(my,.1),(.9+my),my);
wave_1_per_point11=
wave_1_per_point12=x=mx;
wave_1_per_point13=y=my;
wave_1_per_point14=
wave_1_per_point15=a=(above(bass+mid+treb,.1));
wave_1_per_point16=pi23=4*asin(1)*.333333333;
wave_1_per_point17=vol=bass+mid+treb;
wave_1_per_point18=r=(sin(time*.3+vol-0*pi23)+1)*.5;
wave_1_per_point19=g=(sin(time*.3+vol-1*pi23)+1)*.5;
wave_1_per_point20=b=(sin(time*.3+vol-2*pi23)+1)*.5;
wavecode_2_enabled=1
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=0
wavecode_2_bUseDots=1
wavecode_2_bDrawThick=1
wavecode_2_bAdditive=0
wavecode_2_scaling=1.00000
wavecode_2_smoothing=0.50000
wavecode_2_r=1.000
wavecode_2_g=1.000
wavecode_2_b=1.000
wavecode_2_a=1.000
wave_2_per_point1=ma=ma+(above(mid,1)*3.1415*.01*mid);
wave_2_per_point2=ma=ma-(above(treb,1)*3.1415*.01*treb);
wave_2_per_point3=
wave_2_per_point4=mx=mx+(.0004*cos(ma));
wave_2_per_point5=my=my+(.0004*sin(ma));
wave_2_per_point6=
wave_2_per_point7=mx=if(above(mx,.9),(.9-mx),mx);
wave_2_per_point8=my=if(above(my,.9),(.9-my),my);
wave_2_per_point9=mx=if(below(mx,.1),(.9+mx),mx);
wave_2_per_point10=my=if(below(my,.1),(.9+my),my);
wave_2_per_point11=
wave_2_per_point12=x=mx;
wave_2_per_point13=y=my;
wave_2_per_point14=
wave_2_per_point15=a=(above(bass+mid+treb,.3));
wave_2_per_point16=pi23=4*asin(1)*.333333333;
wave_2_per_point17=vol=bass+mid+treb;
wave_2_per_point18=r=(sin(time*.3+vol-0*pi23)+1)*.5;
wave_2_per_point19=g=(sin(time*.3+vol-1*pi23)+1)*.5;
wave_2_per_point20=b=(sin(time*.3+vol-2*pi23)+1)*.5;
wavecode_3_enabled=1
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=0
wavecode_3_bUseDots=0
wavecode_3_bDrawThick=1
wavecode_3_bAdditive=0
wavecode_3_scaling=1.00000
wavecode_3_smoothing=0.50000
wavecode_3_r=1.000
wavecode_3_g=1.000
wavecode_3_b=1.000
wavecode_3_a=1.000
wave_3_per_point1=ma=ma+(above(bass,.5)*3.1415*.02*bass);
wave_3_per_point2=ma=ma-(above(treb,.5)*3.1415*.02*treb);
wave_3_per_point3=
wave_3_per_point4=mx=mx+(.0008*cos(ma));
wave_3_per_point5=my=my+(.0008*sin(ma));
wave_3_per_point6=
wave_3_per_point7=mx=if(above(mx,.9),(.9-mx),mx);
wave_3_per_point8=my=if(above(my,.9),(.9-my),my);
wave_3_per_point9=mx=if(below(mx,.1),(.9+mx),mx);
wave_3_per_point10=my=if(below(my,.1),(.9+my),my);
wave_3_per_point11=
wave_3_per_point12=x=mx;
wave_3_per_point13=y=my;
wave_3_per_point14=
wave_3_per_point15=a=(above(bass+mid+treb,.2));
wave_3_per_point16=pi23=4*asin(1)*.333333333;
wave_3_per_point17=vol=bass+mid+treb;
wave_3_per_point18=r=(sin(time*.3+vol-0*pi23)+1)*.5;
wave_3_per_point19=g=(sin(time*.3+vol-1*pi23)+1)*.5;
wave_3_per_point20=b=(sin(time*.3+vol-2*pi23)+1)*.5;
shapecode_0_enabled=1
shapecode_0_sides=25
shapecode_0_additive=1
shapecode_0_thickOutline=0
shapecode_0_textured=0
shapecode_0_num_inst=34
shapecode_0_x=0.500
shapecode_0_y=0.500
shapecode_0_rad=0.02339
shapecode_0_ang=0.00000
shapecode_0_tex_ang=0.62832
shapecode_0_tex_zoom=1.00000
shapecode_0_r=1.000
shapecode_0_g=1.000
shapecode_0_b=1.000
shapecode_0_a=0.500
shapecode_0_r2=0.000
shapecode_0_g2=0.000
shapecode_0_b2=0.000
shapecode_0_a2=0.500
shapecode_0_border_r=1.000
shapecode_0_border_g=1.000
shapecode_0_border_b=1.000
shapecode_0_border_a=0.000
shape_0_per_frame1=ma=ma+(above(bass,.5)*3.1415*.02*bass);
shape_0_per_frame2=ma=ma-(above(treb,.5)*3.1415*.02*treb);
shape_0_per_frame3=
shape_0_per_frame4=mx=mx+(.002*cos(ma));
shape_0_per_frame5=my=my+(.002*sin(ma));
shape_0_per_frame6=
shape_0_per_frame7=mx=if(above(mx,.9),(.9-mx),mx);
shape_0_per_frame8=my=if(above(my,.9),(.9-my),my);
shape_0_per_frame9=mx=if(below(mx,.1),(.9+mx),mx);
shape_0_per_frame10=my=if(below(my,.1),(.9+my),my);
shape_0_per_frame11=
shape_0_per_frame12=x=mx+instance*.005;
shape_0_per_frame13=y=my+instance*.005;
shape_0_per_frame14=
shape_0_per_frame15=a=(above(bass+mid+treb,.2));
shape_0_per_frame16=pi23=4*asin(1)*.333333333;
shape_0_per_frame17=vol=bass+mid+treb;
shape_0_per_frame18=r=(sin(1/instance*time*.2+vol-0*pi23)+1)*.5;
shape_0_per_frame19=g=(sin(1/instance*time*.2+vol-1*pi23)+1)*.5;
shape_0_per_frame20=b=(sin(1/instance*time*.2+vol-2*pi23)+1)*.5;
shapecode_1_enabled=1
shapecode_1_sides=25
shapecode_1_additive=1
shapecode_1_thickOutline=0
shapecode_1_textured=0
shapecode_1_num_inst=106
shapecode_1_x=0.500
shapecode_1_y=0.500
shapecode_1_rad=0.02248
shapecode_1_ang=0.00000
shapecode_1_tex_ang=0.00000
shapecode_1_tex_zoom=1.00000
shapecode_1_r=1.000
shapecode_1_g=0.000
shapecode_1_b=0.000
shapecode_1_a=0.700
shapecode_1_r2=0.000
shapecode_1_g2=0.000
shapecode_1_b2=0.000
shapecode_1_a2=0.100
shapecode_1_border_r=1.000
shapecode_1_border_g=1.000
shapecode_1_border_b=1.000
shapecode_1_border_a=0.000
shape_1_per_frame1=ma=ma+(above(bass,.7)*3.1415*.03*bass);
shape_1_per_frame2=ma=ma-(above(treb,.7)*3.1415*.03*treb);
shape_1_per_frame3=
shape_1_per_frame4=mx=mx+(.0015*cos(ma));
shape_1_per_frame5=my=my+(.0015*sin(ma));
shape_1_per_frame6=
shape_1_per_frame7=mx=if(above(mx,.9),(.9-mx),mx);
shape_1_per_frame8=my=if(above(my,.9),(.9-my),my);
shape_1_per_frame9=mx=if(below(mx,.1),(.9+mx),mx);
shape_1_per_frame10=my=if(below(my,.1),(.9+my),my);
shape_1_per_frame11=
shape_1_per_frame12=x=mx+instance*.003;
shape_1_per_frame13=y=my+instance*.003;
shape_1_per_frame14=
shape_1_per_frame15=a=(above(bass+mid+treb,.2));
shape_1_per_frame16=pi23=4*asin(1)*.333333333;
shape_1_per_frame17=vol=bass+mid+treb;
shape_1_per_frame18=r=(sin(1/instance*time*.3+vol-0*pi23)+1)*.5;
shape_1_per_frame19=g=(sin(1/instance*time*.4+vol-1*pi23)+1)*.5;
shape_1_per_frame20=b=(sin(1/instance*time*.35+vol-2*pi23)+1)*.5;
shapecode_2_enabled=1
shapecode_2_sides=25
shapecode_2_additive=1
shapecode_2_thickOutline=0
shapecode_2_textured=0
shapecode_2_num_inst=84
shapecode_2_x=0.500
shapecode_2_y=0.500
shapecode_2_rad=0.03030
shapecode_2_ang=0.00000
shapecode_2_tex_ang=0.00000
shapecode_2_tex_zoom=1.00000
shapecode_2_r=1.000
shapecode_2_g=0.000
shapecode_2_b=0.000
shapecode_2_a=0.700
shapecode_2_r2=0.000
shapecode_2_g2=0.000
shapecode_2_b2=0.000
shapecode_2_a2=0.000
shapecode_2_border_r=1.000
shapecode_2_border_g=1.000
shapecode_2_border_b=1.000
shapecode_2_border_a=0.000
shape_2_per_frame1=ma=ma+(above(bass,.3)*3.1415*.05*bass);
shape_2_per_frame2=ma=ma-(above(treb,.3)*3.1415*.05*treb);
shape_2_per_frame3=
shape_2_per_frame4=mx=mx+(.0055*cos(ma));
shape_2_per_frame5=my=my+(.0055*sin(ma));
shape_2_per_frame6=
shape_2_per_frame7=mx=if(above(mx,.9),(.9-mx),mx);
shape_2_per_frame8=my=if(above(my,.9),(.9-my),my);
shape_2_per_frame9=mx=if(below(mx,.1),(.9+mx),mx);
shape_2_per_frame10=my=if(below(my,.1),(.9+my),my);
shape_2_per_frame11=
shape_2_per_frame12=x=mx+instance*.003;
shape_2_per_frame13=y=my+instance*.003;
shape_2_per_frame14=
shape_2_per_frame15=a=(above(bass+mid+treb,.2));
shape_2_per_frame16=pi23=4*asin(1)*.333333333;
shape_2_per_frame17=vol=bass+mid+treb;
shape_2_per_frame18=r=(sin(1/instance*time*.5+vol-0*pi23)+1)*.5;
shape_2_per_frame19=g=(sin(1/instance*time*.8+vol-1*pi23)+1)*.5;
shape_2_per_frame20=b=(sin(1/instance*time*.25+vol-2*pi23)+1)*.5;
shapecode_3_enabled=1
shapecode_3_sides=25
shapecode_3_additive=1
shapecode_3_thickOutline=0
shapecode_3_textured=0
shapecode_3_num_inst=94
shapecode_3_x=0.500
shapecode_3_y=0.500
shapecode_3_rad=0.02248
shapecode_3_ang=0.00000
shapecode_3_tex_ang=0.00000
shapecode_3_tex_zoom=1.00000
shapecode_3_r=0.000
shapecode_3_g=0.000
shapecode_3_b=0.000
shapecode_3_a=0.700
shapecode_3_r2=0.000
shapecode_3_g2=0.000
shapecode_3_b2=0.000
shapecode_3_a2=0.000
shapecode_3_border_r=1.000
shapecode_3_border_g=1.000
shapecode_3_border_b=1.000
shapecode_3_border_a=0.000
shape_3_per_frame1=ma=ma+(above(bass,.11)*3.1415*.07*bass);
shape_3_per_frame2=ma=ma-(above(treb,.11)*3.1415*.07*treb);
shape_3_per_frame3=
shape_3_per_frame4=mx=mx+(.0085*cos(ma));
shape_3_per_frame5=my=my+(.0085*sin(ma));
shape_3_per_frame6=
shape_3_per_frame7=mx=if(above(mx,.9),(.9-mx),mx);
shape_3_per_frame8=my=if(above(my,.9),(.9-my),my);
shape_3_per_frame9=mx=if(below(mx,.1),(.9+mx),mx);
shape_3_per_frame10=my=if(below(my,.1),(.9+my),my);
shape_3_per_frame11=
shape_3_per_frame12=x=mx+instance*.003;
shape_3_per_frame13=y=my+instance*.003;
shape_3_per_frame14=
shape_3_per_frame15=a=(above(bass+mid+treb,.2));
shape_3_per_frame16=pi23=4*asin(1)*.333333333;
shape_3_per_frame17=vol=bass+mid+treb;
shape_3_per_frame18=r=(sin(1/instance*time*.3+vol-0*pi23)+1)*.5;
shape_3_per_frame19=g=(sin(1/instance*time*.4+vol-1*pi23)+1)*.5;
shape_3_per_frame20=b=(sin(1/instance*time*.35+vol-2*pi23)+1)*.5;
per_frame_init_1=spintime = 0;
per_frame_1=basstime = basstime + bass_att*0.03;
per_frame_2=q1 = basstime;
per_frame_3=vol = pow(bass+mid+treb,2);
per_frame_4=basssum = vol;
per_frame_5=
per_frame_6=basstime = if(below(basstime,465),465,basstime);
per_frame_7=
per_frame_8=stickybit = time%2;
per_frame_9=
per_frame_10=//avg vol
per_frame_11=//buffer 1
per_frame_12=volAvg = volAvg + vol*equal(stickybit,1);
per_frame_13=//number of samples 1 or framerate
per_frame_14=sample1 = sample1 + equal(stickybit,1);
per_frame_15=//buffer 2
per_frame_16=volAvg2 = volAvg2 + vol*equal(stickybit,0);
per_frame_17=//number of samples 2
per_frame_18=sample2 = sample2 + equal(stickybit,0);
per_frame_19=
per_frame_20=//transision
per_frame_21=edge = bnot(equal(bit2,stickybit));
per_frame_22=
per_frame_23=volAvg = volAvg - volAvg*edge*stickybit;
per_frame_24=volAvg2 = volAvg2 - volAvg2*edge*equal(stickybit,0);
per_frame_25=
per_frame_26=sample1 = sample1  - sample1*edge*stickybit;
per_frame_27=sample2 = sample2  - sample2*edge*equal(stickybit,0);
per_frame_28=
per_frame_29=//test vol against avg buffer lvl
per_frame_30=diff = if(equal(stickybit,1), (basssum/(volAvg2/sample2)) , 0);
per_frame_31=diff = if(equal(stickybit,0), (basssum/(volAvg/sample1)), diff);
per_frame_32=
per_frame_33=q3 = diff;
per_frame_34=
per_frame_35=bit2 = time%2;
per_frame_36=
per_frame_37=difftime = difftime + diff*0.03;
per_frame_38=q2 = difftime;
per_frame_39=
per_frame_40=//fix a strange error
per_frame_41=difftime = if(above(difftime,2000),0, difftime);
per_frame_42=
per_frame_43=spintime = spintime + bass*0.03*if(equal(state%2,1),1,-1); 
per_frame_44=q8 = spintime;
per_frame_45=
per_frame_46=state = state + above(diff,10);
per_frame_47=
per_frame_48=monitor = spintime;
per_pixel_1=zoom = 1.05 - sin(q3)*0.04;
per_pixel_2=rot =0;// 4.72;
warp_1=`shader_body
warp_2=`{
warp_3=`    float2 d = texsize.zw * 8;
warp_4=`    float3 dx = ( GetBlur1(uv_orig + float2(1,0)*d) - GetBlur1(uv_orig-float2(1,0)*d) );
warp_5=`    float3 dy = ( GetBlur1(uv_orig + float2(0,1)*d) - GetBlur1(uv_orig-float2(0,1)*d) );
warp_6=`
warp_7=`ret.y = tex2d(sampler_fc_main, frac(uv + float2(dx.y,dy.y)*texsize.zw*4)).y;
warp_8=`float2 dither_uv = uv_orig*texsize.xy*texsize_noise_lq.zw * 1.2 + rand_frame.xy;
warp_9=`ret.y += (tex2D(sampler_noise_lq, dither_uv).xyz-0.5) *0.0 - 0.004;
warp_10=`ret = 0;
warp_11=`ret.y = tex2d(sampler_fc_main, frac(uv)).y;
warp_12=`ret.y += (ret.y - GetBlur3(frac(uv)).y -0.03)*.6 - 0.06;
warp_13=`ret.y += GetBlur3(uv_orig).x*0.3;
warp_14=`
warp_15=`ret.z = tex2d(sampler_fc_main,lerp(uv_orig,uv,0.3) + float2(dx.z,dy.z)*texsize.zw*8).z - 0.03;
warp_16=`ret.z += saturate(0.2-GetBlur2(uv).y)*0.1 + GetBlur2(uv_orig).x*0.2;
warp_17=`
warp_18=`}
comp_1=`shader_body
comp_2=`{
comp_3=`    float2 d = texsize.zw*2;
comp_4=`    float3 dx = ( GetBlur1(uv+float2(1,0)*d)-GetBlur1(uv-float2(1,0)*d) );
comp_5=`    float3 dy = ( GetBlur1(uv+float2(0,1)*d)-GetBlur1(uv-float2(0,1)*d) );
comp_6=`ret = lerp(ret,float3(0.4,0.8,0.9),GetBlur1(uv - float2(dx.y,dy.y)*0).z);
comp_7=`
comp_8=`float2 uv_bg = uv - float2(dx.y,dy.y)*texsize.zw*16 + float2(dx.x,dy.x)*0.2;
comp_9=`ret = lerp(ret,1,(GetBlur2(uv_bg)-GetBlur1(uv_bg)*1+GetPixel(uv_bg)*0.9 + (-dx.y + dy.y)*0.4).y*0.8*float3(1.3,1.04,0.4));
comp_10=`
comp_11=`float2 uv_m = uv - float2(dx.x,dy.x)*texsize.zw*8;
comp_12=`ret = lerp(ret, 2*float3(0,0.5,1), GetBlur3(uv_m - float2(dx.y,dy.y)*0.4).x*0.4);
comp_13=`ret = lerp(ret, 2*float3(0.5,1,1), GetBlur2(uv_m - float2(dx.y,dy.y)*0.2).x*0.4);
comp_14=`ret = lerp(ret, 2*float3(1,1,0.8), GetBlur1(uv_m - float2(dx.y,dy.y)*0.1).x*0.2);
comp_15=`ret = lerp(saturate(ret), float3(0,0,0), GetBlur1(uv_m + float2(1,-1)*0.02).x*0.4);
comp_16=`ret = lerp(saturate(ret), float3(1,-0.2,-0.2), GetPixel(uv).x*0.6);
comp_17=`}
