MILKDROP_PRESET_VERSION=201
PSVERSION=2
PSVERSION_WARP=2
PSVERSION_COMP=2
[preset00]
fRating=5.000000
fGammaAdj=1.000
fDecay=1.000
fVideoEchoZoom=1.007
fVideoEchoAlpha=0.500
nVideoEchoOrientation=1
nWaveMode=0
bAdditiveWaves=1
bWaveDots=0
bWaveThick=0
bModWaveAlphaByVolume=1
bMaximizeWaveColor=0
bTexWrap=1
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=0
bDarken=0
bSolarize=0
bInvert=0
fWaveAlpha=0.001
fWaveScale=1.286
fWaveSmoothing=0.630
fWaveParam=0.000
fModWaveAlphaStart=0.710
fModWaveAlphaEnd=1.300
fWarpAnimSpeed=1.459
fWarpScale=2.007
fZoomExponent=1.00000
fShader=0.000
zoom=0.99990
rot=0.00000
cx=0.500
cy=0.500
dx=0.00000
dy=0.00000
warp=0.01000
sx=0.99990
sy=1.00000
wave_r=0.650
wave_g=0.650
wave_b=0.650
wave_x=0.500
wave_y=0.500
ob_size=0.010
ob_r=1.000
ob_g=1.000
ob_b=1.000
ob_a=0.000
ib_size=0.260
ib_r=0.250
ib_g=0.250
ib_b=0.250
ib_a=0.000
nMotionVectorsX=64.000
nMotionVectorsY=48.000
mv_dx=0.000
mv_dy=0.000
mv_l=0.000
mv_r=1.000
mv_g=1.000
mv_b=1.000
mv_a=0.000
b1n=0.000
b2n=0.000
b3n=0.000
b1x=1.000
b2x=1.000
b3x=1.000
b1ed=0.250
wavecode_0_enabled=1
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=0
wavecode_0_bUseDots=0
wavecode_0_bDrawThick=1
wavecode_0_bAdditive=0
wavecode_0_scaling=1.00000
wavecode_0_smoothing=0.50000
wavecode_0_r=1.000
wavecode_0_g=1.000
wavecode_0_b=1.000
wavecode_0_a=1.000
wave_0_per_point1=ma=ma+(above(bass,1)*3.1415*.01*bass);
wave_0_per_point2=ma=ma-(above(treb,1)*3.1415*.01*treb);
wave_0_per_point3=
wave_0_per_point4=mx=mx+(.0002*cos(ma));
wave_0_per_point5=my=my+(.0002*sin(ma));
wave_0_per_point6=
wave_0_per_point7=mx=if(above(mx,.9),(.9-mx),mx);
wave_0_per_point8=my=if(above(my,.9),(.9-my),my);
wave_0_per_point9=mx=if(below(mx,.1),(.9+mx),mx);
wave_0_per_point10=my=if(below(my,.1),(.9+my),my);
wave_0_per_point11=
wave_0_per_point12=x=mx;
wave_0_per_point13=y=my;
wave_0_per_point14=
wave_0_per_point15=a=(above(bass+mid+treb,.8));
wavecode_1_enabled=1
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=0
wavecode_1_bUseDots=0
wavecode_1_bDrawThick=1
wavecode_1_bAdditive=0
wavecode_1_scaling=1.00000
wavecode_1_smoothing=0.50000
wavecode_1_r=1.000
wavecode_1_g=1.000
wavecode_1_b=1.000
wavecode_1_a=1.000
wave_1_per_point1=ma=ma+(above(bass,1)*3.1415*.05*bass);
wave_1_per_point2=ma=ma-(above(mid,1)*3.1415*.05*mid);
wave_1_per_point3=
wave_1_per_point4=mx=mx+(.0001*cos(ma));
wave_1_per_point5=my=my+(.0001*sin(ma));
wave_1_per_point6=
wave_1_per_point7=mx=if(above(mx,.9),(.9-mx),mx);
wave_1_per_point8=my=if(above(my,.9),(.9-my),my);
wave_1_per_point9=mx=if(below(mx,.1),(.9+mx),mx);
wave_1_per_point10=my=if(below(my,.1),(.9+my),my);
wave_1_per_point11=
wave_1_per_point12=x=mx;
wave_1_per_point13=y=my;
wave_1_per_point14=
wave_1_per_point15=a=(above(bass+mid+treb,.1));
wavecode_2_enabled=1
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=0
wavecode_2_bUseDots=1
wavecode_2_bDrawThick=1
wavecode_2_bAdditive=0
wavecode_2_scaling=1.00000
wavecode_2_smoothing=0.50000
wavecode_2_r=1.000
wavecode_2_g=1.000
wavecode_2_b=1.000
wavecode_2_a=1.000
wave_2_per_point1=ma=ma+(above(mid,1)*3.1415*.01*mid);
wave_2_per_point2=ma=ma-(above(treb,1)*3.1415*.01*treb);
wave_2_per_point3=
wave_2_per_point4=mx=mx+(.0004*cos(ma));
wave_2_per_point5=my=my+(.0004*sin(ma));
wave_2_per_point6=
wave_2_per_point7=mx=if(above(mx,.9),(.9-mx),mx);
wave_2_per_point8=my=if(above(my,.9),(.9-my),my);
wave_2_per_point9=mx=if(below(mx,.1),(.9+mx),mx);
wave_2_per_point10=my=if(below(my,.1),(.9+my),my);
wave_2_per_point11=
wave_2_per_point12=x=mx;
wave_2_per_point13=y=my;
wave_2_per_point14=
wave_2_per_point15=a=(above(bass+mid+treb,.3));
wavecode_3_enabled=1
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=0
wavecode_3_bUseDots=0
wavecode_3_bDrawThick=1
wavecode_3_bAdditive=0
wavecode_3_scaling=1.00000
wavecode_3_smoothing=0.50000
wavecode_3_r=1.000
wavecode_3_g=1.000
wavecode_3_b=1.000
wavecode_3_a=1.000
wave_3_per_point1=ma=ma+(above(bass,.5)*3.1415*.02*bass);
wave_3_per_point2=ma=ma-(above(treb,.5)*3.1415*.02*treb);
wave_3_per_point3=
wave_3_per_point4=mx=mx+(.0008*cos(ma));
wave_3_per_point5=my=my+(.0008*sin(ma));
wave_3_per_point6=
wave_3_per_point7=mx=if(above(mx,.9),(.9-mx),mx);
wave_3_per_point8=my=if(above(my,.9),(.9-my),my);
wave_3_per_point9=mx=if(below(mx,.1),(.9+mx),mx);
wave_3_per_point10=my=if(below(my,.1),(.9+my),my);
wave_3_per_point11=
wave_3_per_point12=x=mx;
wave_3_per_point13=y=my;
wave_3_per_point14=
wave_3_per_point15=a=(above(bass+mid+treb,.2));
shapecode_0_enabled=0
shapecode_0_sides=4
shapecode_0_additive=0
shapecode_0_thickOutline=0
shapecode_0_textured=1
shapecode_0_num_inst=1
shapecode_0_x=0.500
shapecode_0_y=0.500
shapecode_0_rad=1.79142
shapecode_0_ang=0.00000
shapecode_0_tex_ang=0.62832
shapecode_0_tex_zoom=1.00000
shapecode_0_r=1.000
shapecode_0_g=1.000
shapecode_0_b=1.000
shapecode_0_a=0.000
shapecode_0_r2=0.000
shapecode_0_g2=0.000
shapecode_0_b2=0.000
shapecode_0_a2=1.000
shapecode_0_border_r=1.000
shapecode_0_border_g=1.000
shapecode_0_border_b=1.000
shapecode_0_border_a=0.000
shapecode_1_enabled=0
shapecode_1_sides=4
shapecode_1_additive=0
shapecode_1_thickOutline=0
shapecode_1_textured=0
shapecode_1_num_inst=1
shapecode_1_x=0.500
shapecode_1_y=0.500
shapecode_1_rad=0.10000
shapecode_1_ang=0.00000
shapecode_1_tex_ang=0.00000
shapecode_1_tex_zoom=1.00000
shapecode_1_r=1.000
shapecode_1_g=0.000
shapecode_1_b=0.000
shapecode_1_a=1.000
shapecode_1_r2=0.000
shapecode_1_g2=1.000
shapecode_1_b2=0.000
shapecode_1_a2=0.000
shapecode_1_border_r=1.000
shapecode_1_border_g=1.000
shapecode_1_border_b=1.000
shapecode_1_border_a=0.100
shapecode_2_enabled=0
shapecode_2_sides=4
shapecode_2_additive=0
shapecode_2_thickOutline=0
shapecode_2_textured=0
shapecode_2_num_inst=1
shapecode_2_x=0.500
shapecode_2_y=0.500
shapecode_2_rad=0.10000
shapecode_2_ang=0.00000
shapecode_2_tex_ang=0.00000
shapecode_2_tex_zoom=1.00000
shapecode_2_r=1.000
shapecode_2_g=0.000
shapecode_2_b=0.000
shapecode_2_a=1.000
shapecode_2_r2=0.000
shapecode_2_g2=1.000
shapecode_2_b2=0.000
shapecode_2_a2=0.000
shapecode_2_border_r=1.000
shapecode_2_border_g=1.000
shapecode_2_border_b=1.000
shapecode_2_border_a=0.100
shapecode_3_enabled=0
shapecode_3_sides=4
shapecode_3_additive=0
shapecode_3_thickOutline=0
shapecode_3_textured=0
shapecode_3_num_inst=1
shapecode_3_x=0.500
shapecode_3_y=0.500
shapecode_3_rad=0.10000
shapecode_3_ang=0.00000
shapecode_3_tex_ang=0.00000
shapecode_3_tex_zoom=1.00000
shapecode_3_r=1.000
shapecode_3_g=0.000
shapecode_3_b=0.000
shapecode_3_a=1.000
shapecode_3_r2=0.000
shapecode_3_g2=1.000
shapecode_3_b2=0.000
shapecode_3_a2=0.000
shapecode_3_border_r=1.000
shapecode_3_border_g=1.000
shapecode_3_border_b=1.000
shapecode_3_border_a=0.100
per_frame_init_1=vol = 0; p1 = 0;
per_frame_init_2=vx = .2; vy = -0.1;
per_frame_init_3=kx = 0; ky = 0;
per_frame_init_4=
per_frame_1=dec_med = pow (0.96, 30/fps);
per_frame_2=dec_slow = pow (0.98, 30/fps);
per_frame_3=beat = max (max (bass, mid), treb); 
per_frame_4=avg = avg*dec_slow + beat*(1-dec_slow);
per_frame_5=is_beat = above(beat, .5+avg+peak) * above (time, t0+.2);
per_frame_6=t0 = is_beat*time + (1-is_beat)*t0;
per_frame_7=peak = is_beat * beat + (1-is_beat)*peak*dec_med;
per_frame_8=index = (index + is_beat) %8;
per_frame_9=index2 = (index2 + is_beat*bnot(index))%2;
per_frame_10=index3 = (index3 + is_beat*bnot(index) * bnot(index2))%2;
per_frame_11=
per_frame_12=q20 = avg;
per_frame_13=q21 = beat;
per_frame_14=q22 = peak;
per_frame_15=q23 = index;
per_frame_16=q24 = is_beat;
per_frame_17=
per_frame_18=vol = bass_att + treb_att;
per_frame_19=v2 = v2 * dec_slow + vol * (1-dec_slow) ;
per_frame_20=q26 = max(atan (vol - v2*.8),.3);
per_frame_21=
per_frame_22=q27 = index + 1;
per_frame_23=
per_frame_24=sw = sw*dec_med + (1-dec_med)*(index2%2);
per_frame_25=q28 = sw;
per_frame_26=
per_frame_27=k1 =  is_beat*bnot(index);
per_frame_28=k2 =  is_beat*bnot(index);
per_frame_29=
per_frame_30=p1 =  k1*(p1+1) + (1-k1)*p1;
per_frame_31=p2 = dec_slow * p2+ (1-dec_slow)*p1;
per_frame_32=rott = p2 * 3.1416/2;
per_frame_33=monitor = k1;
per_frame_34=q1 = cos(rott);
per_frame_35=q2 = sin(rott);
per_frame_36=q3 = -q2;
per_frame_37=q4 = q1;
per_frame_38=
per_frame_39=
per_frame_40=q5 = cos(time/6);
per_frame_41=q6 = -sin(time/6);
per_frame_42=q7 = -q6;
per_frame_43=q8 = q5;
per_frame_44=
per_frame_45=zoom = 1;
per_frame_46=rot = -0;
per_frame_47=
per_frame_48=movez = movez + .0035*(q1+1.1)*30/fps;
per_frame_49=q29 = movez;
per_frame_50=rota = rota + .001*(2-q1)*30/fps;
per_frame_51=q30 = rota;
per_frame_52=q31 = 1 + 16*abs(cos(time*.1));
per_frame_53=q32 = .5*cos(time*.08)/4;
per_frame_54=
per_frame_55=
per_frame_56=
warp_1=`sampler sampler_worms;
warp_2=`float3 color, mus;
warp_3=`float dx,dy;
warp_4=`shader_body {
warp_5=`float2 uv1 = (uv-.2) * aspect.xy;
warp_6=`
warp_7=`
warp_8=`float2 uv6 = uv1;
warp_9=`float z = q29*2*length(uv1)+rand_frame * 32;
warp_10=`float2 d = normalize(uv1);
warp_11=`float2 rs = clamp(tan(z)*d,-8,8);
warp_12=`uv += .004*GetBlur1(uv)*float2 (0,1);//rs/20;
warp_13=`
warp_14=`
warp_15=`uv6 = .4*sin(uv1*18*rand_frame);
warp_16=`mus = .051/(length(uv6));
warp_17=`mus *= float3 (1,.8,.5);
warp_18=`
warp_19=`float3 blur = GetBlur2(frac(uv));
warp_20=`
warp_21=`float3 crisp= tex2D(sampler_main,uv);
warp_22=`
warp_23=`float3 ret1 = crisp - blur*.03 + .15*mus;
warp_24=`float2 uv2 = (uv_orig-.5)-float2(.5,.5+0.1*q25);
warp_25=`
warp_26=`q25 = 1;
warp_27=`ret = q25*(ret1*.99-.02) + (1-q25)* GetPixel(uv_orig);
warp_28=`
warp_29=`}
comp_1=`shader_body
comp_2=`{
comp_3=`    float rad_lq = rad * length(texsize.xy)*0.5;
comp_4=`    float ang_lq = ang;
comp_5=`    float2 uv_temp1 = (uv - 0.5) * texsize.xy;
comp_6=`    float rad_hq = length(uv_temp1);
comp_7=`    float ang_hq = atan2(-uv_temp1.y, uv_temp1.x);
comp_8=`
comp_9=`    float2 uv2 = (uv - 0.5);
comp_10=`    float rad2 = rad_lq*0.8;
comp_11=`    float ang2 = ang_lq * M_INV_PI_2;
comp_12=`
comp_13=`        // ROTATION OVER TIME
comp_14=`        #if 1
comp_15=`          ang2 += time*0.025;   //rotate over time
comp_16=`        #endif
comp_17=`
comp_18=`        // FIN TYPE
comp_19=`        float fins = 3 + floor(rand_preset.z*5.95);
comp_20=`        #if 1     // SHARP FINS
comp_21=`          ang2 = frac(ang2*fins)/fins;
comp_22=`              // ENABLE THIS TO MAKE THE FINS ALTERNATE: (seamless!)
comp_23=`              ang2 = abs(ang2 - 0.5/fins);
comp_24=`        #else     // COSINE FINS - a bit slow
comp_25=`          ang2 = cos(ang2*M_PI_2*fins) * 0.023;
comp_26=`        #endif
comp_27=`
comp_28=`        // RADIAL KALEIDOSCOPING?
comp_29=`        #if 0
comp_30=`          rad2 *= g_fTexSize.z;
comp_31=`            // choose one:
comp_32=`            //rad2 = lerp(rad2, frac(rad2*3)/3.0, 0.5);
comp_33=`            rad2 = cos(rad2*5);
comp_34=`            //rad2 = sqrt(rad2)*0.5;
comp_35=`            //rad2 += abs(frac(rad2*7)-0.5)/7.0 * 1.15;  // stepifier
comp_36=`            //rad2 += cos(rad2*61)*0.02;
comp_37=`          rad2 *= g_fTexSize.x;
comp_38=`        #endif
comp_39=`
comp_40=`    ang2 *= M_PI_2;
comp_41=`    uv2 = 0.5 + rad2*float2(cos(ang2),sin(ang2))*texsize.zw;
comp_42=`
comp_43=`    ret = tex2D(sampler_main,uv2).y*float3(0.6,0.2,1.5) + tex2D(sampler_fw_main,uv2).x*float3(1,0.66,0) - tex2D(sampler_main,uv2).z*float3(-0.6,1,2);
comp_44=`}
